Replace potentiometer with hall sensor, then couple to LCD screen for output

